#### $#K OrCAD

CAMCAD Read/Import NameR-OrCAD

Full CAD Format NameOrCAD PCB

Hardware PlatformPC

Operating SystemDOS

Database ClassNet: Connections are allowed to be made in any order and “T” connections are also allowed. Although rules must be followed for trace routing and via placement they are usually very loose, thus allowing the designer much more freedom in the routing process.

Board Outline ClassPseudo: Board outlines in this CAD format are comprised of standard line elements. The CAD format does not allow for a real board outline entity.

Importing OrCAD into CAMCAD

File(s) Used For Import

.MIN (ASCII)

How To Produce File(s)

EXPORT MASSTECK ASCII

Notes On File Generation

To generate the proper .MIN file, under options, “all of the above” should be selected, which is the default setting.

Items controlled by the Orcadltd.IN file

.WIDTH_IN_MIL